<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<packages>
<package name="ESP32WROOM32">
</package>
</packages>
<symbols>
<symbol name="ESP32WROOM32">
<pin name="GND"/>
<pin name="3V3"/>
<pin name="EN"/>
<pin name="SENSOR_VP"/>
<pin name="SENSOR_VN"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO14"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="SD2"/>
<pin name="SD3"/>
<pin name="CMD"/>
<pin name="CLK"/>
<pin name="SD0"/>
<pin name="SD1"/>
<pin name="IO15"/>
<pin name="IO2"/>
<pin name="IO0"/>
<pin name="IO4"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO5"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="NC"/>
<pin name="IO21"/>
<pin name="RXD0"/>
<pin name="TXD0"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="THERM"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ESP32">
<description>ESP32-WROOM-32 is a powerful, generic Wi-Fi+BT+BLE MCU module that targets a wide variety of
applications, ranging from low-power sensor networks to the most demanding tasks, such as voice encoding,
music streaming and MP3 decoding.</description>
<gates>
<gate name="ESP32" symbol="ESP32WROOM32"/>
</gates>
<devices>
<device name="" package="ESP32WROOM32">
<connects>
<connect gate="ESP32" pin="3V3" pad="2"/>
<connect gate="ESP32" pin="CLK" pad="20"/>
<connect gate="ESP32" pin="CMD" pad="19"/>
<connect gate="ESP32" pin="EN" pad="3"/>
<connect gate="ESP32" pin="GND" pad="1 15 38"/>
<connect gate="ESP32" pin="IO0" pad="25"/>
<connect gate="ESP32" pin="IO12" pad="14"/>
<connect gate="ESP32" pin="IO13" pad="16"/>
<connect gate="ESP32" pin="IO14" pad="13"/>
<connect gate="ESP32" pin="IO15" pad="23"/>
<connect gate="ESP32" pin="IO16" pad="27"/>
<connect gate="ESP32" pin="IO17" pad="28"/>
<connect gate="ESP32" pin="IO18" pad="30"/>
<connect gate="ESP32" pin="IO19" pad="31"/>
<connect gate="ESP32" pin="IO2" pad="24"/>
<connect gate="ESP32" pin="IO21" pad="33"/>
<connect gate="ESP32" pin="IO22" pad="36"/>
<connect gate="ESP32" pin="IO23" pad="37"/>
<connect gate="ESP32" pin="IO25" pad="10"/>
<connect gate="ESP32" pin="IO26" pad="11"/>
<connect gate="ESP32" pin="IO27" pad="12"/>
<connect gate="ESP32" pin="IO32" pad="8"/>
<connect gate="ESP32" pin="IO33" pad="9"/>
<connect gate="ESP32" pin="IO34" pad="6"/>
<connect gate="ESP32" pin="IO35" pad="7"/>
<connect gate="ESP32" pin="IO4" pad="26"/>
<connect gate="ESP32" pin="IO5" pad="29"/>
<connect gate="ESP32" pin="NC" pad="32"/>
<connect gate="ESP32" pin="RXD0" pad="34"/>
<connect gate="ESP32" pin="SD0" pad="21"/>
<connect gate="ESP32" pin="SD1" pad="22"/>
<connect gate="ESP32" pin="SD2" pad="17"/>
<connect gate="ESP32" pin="SD3" pad="18"/>
<connect gate="ESP32" pin="SENSOR_VN" pad="5"/>
<connect gate="ESP32" pin="SENSOR_VP" pad="4"/>
<connect gate="ESP32" pin="THERM" pad="T T2 T3 T4 T5 T6 T7 T8 T9"/>
<connect gate="ESP32" pin="TXD0" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
